**1. Install patrol system**

Put patrolling the software CD in the computer, install the setup file, after installed, computer desktop icon will appear patrolling system, click the patrolling system, do not need to enter the password, was determined directly, can enter the patrolling system, in this way, patrolling system installation is complete.

**Two, clear out the best data**

Connect the patrol stick with the computer with the data cable. Open the patrol system. First, clear the data inside the patrol stick. Specific steps are: click the patrolling system interface to download data, click on the download data, after the download is complete, click the delete data, red light, said after the data on the tour better delete completed - > click on the back. Click the system Settings - > click parameter Settings - > click while reading time and school (because the time patrolling rod is follow the computer time, computer time right then patrolling rod is correct) - > click on the back. Then click system Settings - click data initialization, click all options, so that all the data in the patrol bar is empty.

**3. Patrol point setting**

To label patrolling point paper and, after the tour more drawing, and then more points, in order to read tour finished, cable to connect computers and patrolling rod, open the patrolling system interface - > basic Settings - > click click site Settings - > click on the data collected, and then under the name will appear in turn checking point 1 and point 2............ Name the patrol points in the name column in order to read the patrol points, and then click return. The system will automatically default to what the patrol is called, and then install these patrol points where they need to be patrolled. The number cannot be changed.

**4. Personnel button setting (no need to set without personnel button)**

The button label paper and naming, the patrolling drawing, and then in order to read button, after reading, cable to connect computers and patrolling rod, open the patrolling system interface - > basic Settings - > Settings - > click on personnel click click to collect data, then under the name will appear in turn 1, personnel 2............ Name these people 1 and 2 in the name column in order to read the person button, and then directly click return. After tour better read it before you clock button, and then to read the patrolling point, the system will automatically default this patrol point is who will go to, then put these button to patrol personnel, each one a, number cannot be modified.

**5. Patrol bar arrangement**

Open the patrolling system interface, the tour more stick label paper and named - > basic Settings - > click click bar Settings - > click collect data, and then the name will appear below number, this number is named patrolling the name of the bar, and then directly point returns. After the patrol is better, the system will automatically default to the patrol better name, and then send the patrol better to the patrol personnel. If there are more than one patrol, it's the same method setting.、

**6. Circuit setting (no plan is required for this place)**

Interface - > click open the patrolling system Settings - > Settings - > click line click add to input line name and click save, click on their name line name - > click on the selection of the patrolling point shift to the left (can choose according to their own requirements need to shift to the left of the point) and then shut down the interface.

**7. Plan setting (there is no need to plan this place)**

Open the patrolling system basic click Settings - > project Settings - > interface - > click on the select routes, choose start time and end time, and then fill in the inspection time, if the inspection time is one hour, then fill in 60 minutes, time and rest time, fixed time, error request order don't need to choose, just click generate plans, click back. If you have a plan time to make, set it the same way.

**Note: if you do not need to make a plan, you only need to check the patrol record after the patrol is finished. Then, the six or seven steps above do not need to be set.**

**These are the setup steps for all patrol systems**

**The following are the administrative staff query and statistics patrol better operation steps**

Patrols after play CARDS, patrolling rod needs to your manager, management personnel to open the patrolling system, cable connection patrolling rod and computer - click on the download data - analysis - click return - click click download data (concrete analysis which period of time, you can choose) analysis is completed, click on the return. Then click the inspection examination to click the data query, and the specific data after analysis will appear. The specific time period can be selected to query. If there are more than one patrol that is better, then each patrol that is better needs to operate in the above way. You can then generate EXCEL and print previews to save your computer and print directly.

If you don't need to make plans, only need to clock in patrol the streets, they can query to the patrol record, such steps are: open the patrolling interface to download data to download data, click on the back. In the interface of patrol system, click inspection record, click data query, and the specific data analyzed will appear. Can choose specific time, query. If there are more than one patrol that is better, then each patrol that is better needs to operate in the above way. You can then generate EXCEL and print previews to save your computer and print directly.

**Backup database**

In order to prevent the computer reshipment system leads to tour more uninstall or accidentally put all initialization data, we can backup the database, such as long as there is a database file, then I can restore, so there is no need to reset the patrolling spot, personnel, plan and other information. Here's how to do it: create a folder on your desktop, open the patrol system interface, click system Settings, click on the backup database, and save it in the folder you created on your desktop. This folder is then placed on a usb drive to back up or on a disk outside of your computer's C drive. Later the patrol system is lost. After installing the patrol system, you can restore this file to the patrol system.

**Patrol better data needs to be cleaned up regularly**

The data stored in patrol bar is limited. If it is not cleaned regularly, the data will be downloaded for a longer time in the future if it is not cleaned regularly. After the data stored in patrol bar is full, the card cannot be read. Specific steps to clear data: open patrol system, click to read data, click to download data, and click to delete data. When patrol is better and the red light is on, it means that patrol data is cleaned up. (remember, empty before tour better, if the data again to retain backup before clearance) all over a data point, will be saved in patrolling inspection records in the interface, and this is not the tour more wonderful memory.